Thanks for purchasing PLANET GS-6320-24UP2T2XV L3 24-Port 10/100/1000T 802.3bt PoE + 2-Port 10GBASE-T + 2-Port 10G SFP+ Managed Switch with LCD Touch Screen and Redundant Power.

Please note that this firmware version is for GS-6320-24UP2T2XV hardware version 2. 

This document provides the firmware release note and history of the product below:

v2.2412b251121

Version v2.2412b251121 was released on 12/19/2025
=======================================
Firmware version: v2.2412b251121
Hardware version: 2.0
File Name: FW-GS-6320-24UP2T2XV_v2.2412b251121.mfi
File Size: 18,474,328 bytes
Released on 12/19/2025
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Functions added
          Supports CloudNMS function


******************************
Firmware Release History:  
******************************

Version v2.2112b240523 was released on 05/27/2024
=======================================
Firmware version: v2.2112b240523
Hardware version: 2.0
File Name: FW-GS-6320-24UP2T2XV_v2.2112b240523.mfi
File Size: 17,957,045 bytes
Released on 05/27/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Functions added
          Supports PSTI Act to enhance product security

          (Default login authentication for the device are username: admin and password: sw + the last 6 characters of the MAC ID in lowercase)


Version v2.2112b230704 was released on 07/04/2023
=======================================
Firmware version: v2.2112b230704
Hardware version: 2.0
File Name: 
File Size: 
Released on 07/04/2023
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Functions - N/A

     Initial Release.

[Note]
Hardware-based factory reset default is required for this firmware upgrade.
Press the hardware-based reset button on the device for about 10 seconds. 

[Upgrade Requirements]:

1. The latest firmware version of GS-6320-24UP2T2XV.
2. The GS-6320-24UP2T2XV switch.
3. Workstation with Google Chrome, Microsoft Edge or Mozilla Firefox.

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click Maintenance--> Web Firmware Upgrade" on the left side of the Menu.  

     Web Firmware Upgrade:
     (1) Click the "Choose File" button to locate firmware path.
     (2) Click the "Upload" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the firmware upgrade process is completed.
     (4) Reset to factory default and reboot system again.

4. Relogin the switch via Web browser. Please click "System -->System Information --> Software Version" to double-check if the firmware is upgraded successfully.


   
Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw

