Thanks for purchasing PLANET GS-6320-46S2C4XR L3 46-Port 100/1000BASE-X SFP + 2-Port Gigabit TP/SFP + 4-Port 10G SFP+ Managed Switch.

This document contains the firmware release note and history for the following product:

Version 1.440b240515 was released on 15/5/2024
=======================================
Firmware version: v1.440b240515
Hardware version: 1.0
File Name: FW-GS-6320-46S2C4XR_v1.440b240515.mfi
File Size: 14,557,184 bytes 
Released on 15/5/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed -N/A

B: Function added or enhanced
    1. Supports PSTI Act to enhance product security.
       (Default login authentications for the device are username: "admin" and password: "sw + the last 6 characters of the MAC ID in lowercase".)
   
[Note]
Hardware-based factory reset default is required for this firmware upgrade.
Press the hardware-based reset button on the device for about 10 seconds. 

[Upgrade Requirements]:

1. The latest firmware version of GS-6320-46S2C4XR.
2. The GS-6320-46S2C4XR Switch.
3. Workstation with Microsoft Edge, Google Chrome or Firefox.

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click Maintenance--> Web Firmware Upgrade" on the left side of the Menu.  

     Web Firmware Upgrade:
     (1) Click the "Choose File" button to locate firmware path.
     (2) Click the "Upload" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the firmware upgrade process is completed.
     (4) Reset to factory default and reboot system again.

4. Relog in to the switch via Web browser. Please click "System -->System Information --> Software Version" to double-check if the firmware is upgraded successfully.

******************************
Firmware Release History:  
******************************
=======================================
Version 1.440b210505 was released on 5/5/2021
=======================================
Firmware version: v1.440b210505
Hardware version: 1.0
File Name: FW-GS-6320-46S2C4XR_v1.440b210505.mfi
File Size: 14,057,472 bytes 
Released on 5/5/2021
=======================================

This firmware provides the following modifications:

A: Bug Fixed
   1. Fixed Switch Port link down/link up issue.

B: Function added  - N/A

=======================================
Version 1.440b201019 was released on 19/10/2020
=======================================
Firmware version: v1.440b201019
Hardware version: 1.0
File Name: FW-GS-6320-46S2C4XR_v1.440b201019.mfi
File Size: 14,041,088 bytes 
Released on 19/10/2020
=======================================

This firmware provides the following modifications:

A: Bug Fixed
   1. Fixed MGB-GT SFP copper module not link after switch reboot issue.

B: Function added  - N/A

=======================================
Version 1.440b200521 was released on 21/5/2020
=======================================
Firmware version: v1.440b200521
Hardware version: 1.0
File Name: FW-GS-6320-46S2C4XR_v1.440b200521.mfi
File Size: 14,475,264 bytes 
Released on 21/5/2020
=======================================

This firmware provides the following modifications:

A: Bug Fixed
   1. Fixed copper port LEDs not lit on issue.

B: Function added  - N/A

=======================================
Version 1.440b200504 was released on 4/5/2020
=======================================
Firmware version: v1.440b200504
Hardware version: 1.0
File Name: FW-GS-6320-46S2C4XR_v1.440b200504.mfi
File Size: 14,479,360 bytes 
Released on 4/5/2020
=======================================

Initial Release

Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw









