Thanks for purchasing PLANET MGSD-10080F 6-Port 100/1000X SFP + 2-Port 1G/2.5G SFP + 2-Port 10/100/1000T Managed Metro Ethernet Switch.

Please note that this firmware version is for MGSD-10080F hardware version 2. 

This document provides the firmware release note and history of the product below:

Version 2.2412b260422 was released on 22/4/2026
=======================================
Firmware version: v2.2412b260422
Hardware version: 2.0
File Name: FW-MGSD-10080F_v2.2412b260422.mfi
File Size: 17,858,560 bytes 
Released on 22/4/2026
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
   NA.
   
B. Function Added -
    1. Support PLANET CloudNMS.

C. Other:
   NA.

D: Other
    1.Firmware SDK upgrade to IStaX 24.12.
   
[Note]
Hardware-based factory reset default is required for this firmware upgrade.
Press the hardware-based reset button on the device for about 10 seconds. 

[Upgrade Requirements]:

1. The latest firmware version of MGSD-10080F.
2. The MGSD-10080F switch.
3. Workstation with web browser tools.

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click Maintenance--> Web Firmware Upgrade" on the left side of the Menu.  

     Web Firmware Upgrade:
     (1) Click the "Choose File" button to locate firmware path.
     (2) Click the "Upload" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the firmware upgrade process is completed.
     (4) Reset to factory default and reboot system again.

4. Relog in the switch via Web browser. Please click "System -->System Information --> Software Version" to double-check if the firmware is upgraded successfully.


******************************
Firmware Release History:  
******************************
=======================================
Version 2.440b240318 was released on 18/3/2024
=======================================
Firmware version: v2.440b240318
Hardware version: 2.0
File Name: FW-MGSD-10080F_v2.440b240318.mfi
File Size: 14,389,248 bytes 
Released on 18/3/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed-NA

B: Function added or enhanced
    1. Supports PSTI Act to enhance product security
       (Default login authentications for the device are username: "admin" and password: "sw + the last 6 characters of the MAC ID in lowercase".)

=======================================
Version 2.440b220314 was released on 14/3/2022
=======================================
Firmware version: v2.440b220314
Hardware version: 2.0
File Name: FW-MGSD-10080F_v2.440b220314.mfi
File Size: 13,975,552 bytes 
Released on 14/3/2022
=======================================

This firmware provides the following modifications:

A: Bug Fixed
    1. Fix SSH Login Issue.
    2. Fix NMS Device Description display issue.

B: Function added - NA

=======================================
Version .440b210610 was released on 10/6/2021
=======================================
Firmware version: v2.440b210610
Hardware version: 2.0
File Name: FW-MGSD-10080F_v2.440b210610.mfi
File Size: 13,869,056 bytes 
Released on 10/6/2021
=======================================

Initial Release
   
Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw







