Thanks for purchasing PLANET IGS-10020MT Industrial L2+ 8-port 10/100/1000T + 2-port 1G/2.5G SFP Managed Gigabit Switch.

Please note that this firmware version is for the IGS-10020MT hardware version 3 only. You can get the information from the serial number. 
When you see the model name on the serial number which is the IGS-10020MT (v3), it is hardware version 3. If the model name is the IGS-10020MT(v2), it is hardware version 2. 

This document provides the firmware release note and history of the product below:

Version 3.440b240326 was released on 26/3/2024
=======================================
Firmware version: v3.440b240326
Hardware version: 3.0
File Name: FW-IGS-10020MT_v3.440b240326.mfi
File Size: 14,467,072 bytes 
Released on 26/3/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed -N/A

B: Function added or enhanced
    1. Supports PSTI Act to enhance product security
       (Default login authentications for the device are username: "admin" and password: "sw + the last 6 characters of the MAC ID in lowercase".)

[Note]
Hardware-based factory reset default is required for this firmware upgrade.
Press the hardware-based reset button on the device for about 10 seconds. 

[Upgrade Requirements]:

1. The latest firmware version of IGS-10020MT.
2. The IGS-10020MT switch.
3. Workstation with web browser tools..

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click Maintenance--> Web Firmware Upgrade" on the left side of the Menu.  

     Web Firmware Upgrade:
     (1) Click the "Choose File" button to locate firmware path.
     (2) Click the "Upload" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the firmware upgrade process is completed.
     (4) Reset to factory default and reboot system again.

4. Relogin the switch via Web browser. Please click "System -->System Information --> Software Version" to double-check if the firmware is upgraded successfully.



******************************
Firmware Release History:  
******************************

Version 3.440b200817 was released on 08/21/2020
=======================================
Firmware version: v3.440b200817
Hardware version: 3.0
File Name: FW-IGS-10020MT_v3.440b200817.mfi
File Size: 13,892,965 bytes 
Released on 08/21/2020
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Function added - 

    1. Added PLANET CloudViewer app support.



Version 3.440b200722 was released on 07/22/2020
=======================================
Firmware version: v3.440b200722
Hardware version: 3.0
File Name: FW-IGS-10020MT_v3.440b200722.mfi
File Size: 14,352,384 bytes 
Released on 07/22/2020
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Function added - 

   1. Added port 9 and port 10 that support an operating speed of 2.5G.



Version 3.440190919 was released on 02/26/2020
=======================================
Firmware version: v3.440190919
Hardware version: 3.0
File Name: FW-IGS-10020MT_v3.440190919.mfi
File Size: 13,659,489 bytes 
Released on 09/19/2019
=======================================

This firmware provides the following modifications:

A: Bug Fixed -

   1. Fixed Ethernet port 10Mbps half duplex communication situation.

B: Function added - N/A


Version 3.440181106 was released on 11/06/2018
=======================================
Firmware version: V3.440181106
Hardware version: 3.0
File Name: FW-IGS-10020MT_v3.440181106.mfi
File Size: 13,839,713 bytes 
Released on 11/06/2018
=======================================

Initial Release
   
Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw







